# Tolerance Analysis Report

Report Generated On Tue May 13 2008 @ 02:53:18 pm
Analysis Report By:
Company :

Derivative-Based Statistical Analysis

#### Measure Details

ProE Nominal and Tolerance | 1.000/0.000
Solved Nominal | 0.15
Standard Deviation | 0.0810807
Worst Case Range : | Max = 0.9 Min = -0.5

#### Sensitivity and Statistical Contribution Details

Name: | Dim./Tolerance: | Cp | Sensitivity | Variance/Contribution
--- | --- | --- | --- | ---
PAN:d39 | 146.0 ±0.1 | 1.00 | 1 |
| 16.90%
PAN:d8 | |POS|0.2|MMC| | 1.00 | -1 |
| 16.90%
PCB:d266 | 25.00 ±0.10 | 1.00 | -1 |
| 16.90%
PCB:d43 | 7.10 ±0.10 | 1.00 | 1 |
| 16.90%
REC-3PIN:d137 | |POS|0.2| | 1.00 | -1 |
| 16.90%
PAN/SCREW:Clearance | 0.150/-0.150 | 0.00 | 1 |
| 12.71%
SCREW:d1 | 3.4 +0.0/-0.1 | 1.00 | -0.5 |
| 1.39%
PCB:d267 | 3.50 +0.10/0.00 | 1.00 | 0.5 |
| 1.06%
PAN:d9 | 3.5 +0.1/0.0 | 1.00 | 0 |
| 0.33%

Dimension Loop Diagram